**CDH Software**

**Beacon Test Document**

|  |  |
| --- | --- |
| **Prepared by** | Chris Zhang |
| **Revision** | 1.0 |
| **Date** | 2016.02.13 |
| **Reference** | Comm Control Test Document |
| **Signed By** |  |

# Document Change Log

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Description of Changes** | | | **Modified Section** | **Revision** | **Date** | |
| Initial Issue | | |  | 1.0 | 2016.02.13 | |
|  | | |  |  |  | |
|  | | |  |  |  | |
|  |  | | | |

# Procedures

**(To be used in conjunction with the PUS Service Interfaces document, and the Command Line Interface document)**

1. Set up one transceiver with one SSM
2. Put the transceiver to UHF\_Beacon mode
3. Transmit a dummy message
4. Use SDR to receive it
5. Repeat 1-4

# Test Results

Report the results of each major test here and the actions that were taken to correct any issues (or simply insert a link to the issue that was opened)