**Antenna Deployment Code**

* Service Type: 69, service sub type: 13.
* It would be ideal if we had a button with the title “deploy” which could be used to send the required command to the satellite.
* **Need the groundstation code to create the outgoing PUS packet and the satellite’s OPR to act on it and route the action to the EPS board.**
* Tm\_to\_downlink 🡪 tc\_to\_uplink in the GSSW.
* Created setup\_deploy\_command() to create the required telecommand.
* I’m adding a new character to signify the start of a telecommand: !
* Key word: ANT\_DEP causes the antenna to deploy.