**CDH Software**

**Event Reporting Test Document**

|  |  |
| --- | --- |
| **Prepared by** | Keenan Burnett |
| **Revision** | 1.0 |
| **Date** | 2016.01.08 |
| **Reference** | Event Reporting Test Document |
| **Signed By** | Keenan Burnett |

# Document Change Log

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Description of Changes** | | | **Modified Section** | **Revision** | **Date** | |
| Initial Issue | | |  | 1.0 | 2016.01.08 | |
|  | | |  |  |  | |
|  | | |  |  |  | |
|  |  | | | |

# Procedures

**(To be used in conjunction with the PUS Service Interfaces document)**

1. **Reporting Events**
   1. Cause some action on the satellite to create one of each of the kinds of error reports (normal, low-sev error, medium-sev error, high-sev error)
   2. Verify that the GSSW parses them and places them into the event log properly under /events/. Make sure that each of the lines makes sense and has no syntax errors.

# Test Results

Report the results of each major test here and the actions that were taken to correct any issues (or simply insert a link to the issue that was opened)